

Technical Notice – DIM10-087-06-A

DIM10-087-06-A revisions K-0 and higher have new wire colors to comply with the National Electric Code (NEC) recommendations for low voltage dimming. Also, the

DIM-/COMMON wire was eliminated because it is duplicated by the DALI-/COMMON wire.

|  |  |  |
| --- | --- | --- |
| **Signal Name** | **Old Color** | **New Color** |
| DALI-/COMMON | BROWN | PINK/WHITE STRIPE |
| DALI+ | YELLOW | VIOLET/WHITE STRIPE |
| DIM+ | VIOLET | VIOLET |
| DIM-/COMMON | BLACK | *Removed* |
| SENSOR INPUT B | ORANGE | ORANGE |
| SENSOR INPUT A | BLUE | YELLOW |
| POWER | RED | BROWN |